Universidad del Valle de Guatemala

Electrónica Digital II

Rodrigo Díaz, 18265

Lab #1

# Pseudocódigo

# Código Documentado

/\*

\* File: main.c

\* Author: Rodrigo Díaz

\*

\*/

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Importación de librerías

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#include <xc.h>

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Palabra de configuración

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// CONFIG1

#pragma config FOSC = XT // Oscillator Selection bits (XT oscillator: Crystal/resonator on RA6/OSC2/CLKOUT and RA7/OSC1/CLKIN)

#pragma config WDTE = OFF // Watchdog Timer Enable bit (WDT disabled and can be enabled by SWDTEN bit of the WDTCON register)

#pragma config PWRTE = OFF // Power-up Timer Enable bit (PWRT disabled)

#pragma config MCLRE = OFF // RE3/MCLR pin function select bit (RE3/MCLR pin function is digital input, MCLR internally tied to VDD)

#pragma config CP = OFF // Code Protection bit (Program memory code protection is disabled)

#pragma config CPD = OFF // Data Code Protection bit (Data memory code protection is disabled)

#pragma config BOREN = OFF // Brown Out Reset Selection bits (BOR disabled)

#pragma config IESO = OFF // Internal External Switchover bit (Internal/External Switchover mode is disabled)

#pragma config FCMEN = OFF // Fail-Safe Clock Monitor Enabled bit (Fail-Safe Clock Monitor is disabled)

#pragma config LVP = OFF // Low Voltage Programming Enable bit (RB3 pin has digital I/O, HV on MCLR must be used for programming)

// CONFIG2

#pragma config BOR4V = BOR40V // Brown-out Reset Selection bit (Brown-out Reset set to 4.0V)

#pragma config WRT = OFF // Flash Program Memory Self Write Enable bits (Write protection off)

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Variables

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// la variable XTAL FREQ es necesaria para que funcionen los delays

#define \_XTAL\_FREQ 8000000

// Se asginan variables de Leds a los primeros 3 bits del puerto E

#define LED\_Rojo PORTEbits.RE0

#define LED\_Amarillo PORTEbits.RE1

#define LED\_Verde PORTEbits.RE2

// se crean variables tipo char que se utilizaran en el programa

unsigned char check = 0;

unsigned char j1 = 0;

unsigned char j2 = 0;

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Prototipos de funciones

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

void setup(void);

void semaforo(void);

void avance(void);

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Ciclo principal

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

void main(void) {

// mando a llamar a la funcion de setup

setup();

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Loop principal

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// como es un while(1) siempre se va a repetir este loop.

while (1) {

// se tiene un antirebote para el boton que activa el semáforo

if (PORTBbits.RB0 == 0) {

\_\_delay\_ms(50);

if (PORTBbits.RB0 == 1) {

// se manda a llamar primero al semaforo y después a la funcion

// de avance para que participen los jugadores

semaforo();

avance();

}

}

}

}

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Configuración

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

void setup(void) {

// Todos los bits utilizados se configuran como salidas, menos los primeros

// 3 bits del puerto B, debido a que allí estan los push. Ansel y Anselh

// se ponen en 0 porque no se utilizarán señales analógicas.

TRISE = 0;

PORTE = 0;

ANSEL = 0;

ANSELH = 0;

TRISB = 0b00000111;

PORTB = 0;

TRISC = 0;

PORTC = 0;

TRISD = 0;

PORTD = 0;

PORTA = 0;

TRISA = 0;

}

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

// Funciones

//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

void semaforo(void) {

// Al inicio del juego, todos los puertos que involucren los LEDs de los

// jugadores se apagan.

PORTC = 0;

PORTD = 0;

PORTA = 0;

// Se encienden los colores del semáforo con un delay especificado

LED\_Rojo = 1;

\_\_delay\_ms(150);

LED\_Rojo = 0;

LED\_Amarillo = 1;

\_\_delay\_ms(150);

LED\_Amarillo = 0;

LED\_Verde = 1;

\_\_delay\_ms(150);

LED\_Verde = 0;

// la variables check se enciende para poder comenzar a contar el punteo

check = 1;

}

void avance(void) {

// solamente si check es 1, se puede entrar al loop

while (check == 1) {

// se tiene un antirebote para el botón del jugador 1

if (PORTBbits.RB1 == 0) {

\_\_delay\_ms(50);

if (PORTBbits.RB1 == 1) {

// se revisa si es su primer botonazo para encender el primer

// LED, sino solo hace un corrimiento de bits. Una vez se llega

// al octavo LED, se apaga check para que no se pueda seguir

//jugando y se enciente el LED que ganó el jugador 1.

if (PORTC == 0) {

j1 = 0b00000001;

PORTC = j1;

}

else if (PORTC != 0) {

j1 = j1\*2;

PORTC = j1;

}

if (PORTCbits.RC7 == 1) {

check = 0;

PORTAbits.RA0 = 1;

}

}

}

// antirebote para el jugador 2

if (PORTBbits.RB2 == 0) {

\_\_delay\_ms(50);

if (PORTBbits.RB2 == 1) {

// tiene la misma estructura que para el jugador 1, pero con

//los puertos y variables del jugador 2

if (PORTD == 0) {

j2 = 0b00000001;

PORTD = j2;

}

else if (PORTD != 0) {

j2 = j2\*2;

PORTD = j2;

}

if (PORTDbits.RD7 == 1) {

check = 0;

PORTAbits.RA1 = 1;

}

}

}

}

}

# Link Repositorio Github